Do you have this problem?
The Okki Nokki stops working suddenly. Both motors do not work anymore. After a while the Okki is in some occasions working again for a short period.

Probably the sensor in the reservoir is dirty.

A simple solution is to disconnect this sensor from the harness inside the machine. There is a small connector coming from the sensor that is placed in the reservoir, to the wire harness. Please disconnect this connector at the harness side and leave it that way.

The float system will not work anymore, but the machine will work perfectly. You have to empty the reservoir after cleaning about 30 records.

When you are a bit technical you can do this job yourself. When you are not able to do it, please go to your nearest dealer or contact your distributor.

The sensor is giving wrong information to the electronic float control devise that is built in the Okki Nokki. It is a devise that stops both motors, when the reservoir is too full with sewage water. We have it in the Okki Nokki to prevent that people who totally do not know what they are doing, are getting water on their table, when the reservoir is over floating.... It has nothing to do with safety, in our system, the water can never come in the vacuum motor. It is the same as writing in a microwave manual that you are not allowed to put your dog in the microwave to dry, because it then dies.... this just to explain, we can live easy without the float control system... As long as you empty the reservoir after each 30 cleaned records.

When you do want to do the job yourself, then here a quick explanation;

*) We are not responsible for not disconnecting the power cable from the Okki Nokki, before and during the change / work on the Okki Nokki!!! DANGER! Not disconnecting the Okki Nokki from the electricity network / grid, can course serious electrical shock!!! You can get a deadly shock! DANGER! There are parts inside the Okki Nokki that have open contacts with 230 volt on them! 
[bookmark: _GoBack]*) After disconnecting the Okki Nokki from the power by pulling out the powercord, at the back of the Okki Nokki, there will be no power on the parts inside anymore.
*) Off course we are responsible for the change, disconnecting the sensor inside the Okki Nokki. You will not lose your warranty on the machine.

1. First remove the powercord from the Okki Nokki! There should not be electrical power to the Okki Nokki when you open the machine / when the machine is opened. You would get an electrical shock!!! DANGER!
1. Remove the sewage fluid from the reservoir, described in the manual.
1. Turn the Okki Nokki upside down. Make shore something soft like a hand towel is under the Okki Nokki to prevent the Okki is damaging or the table is damaging.
1. Unscrew the 4 feet from the bottom plate.
1. Unscrew the 2 small screws in the middle of the bottom plate.
1. Remove the plastic black ventilation cover from the bottom plate. 
1. Remove the bottom plate by putting your fingers in the hole of the ventilation cover. You might have to use force! Do not be afraid to use force! You cannot damage anything. DO not worry. The Okki is very strongly build.
1. Inside the Okki Nokki you see a cable that is coming from the reservoir. The cable is going thru the side wall and then is coming into the dry department. On the end of this cable there is a small black connector. This connector is connected to the wire harness. Disconnect this small black connector and the Okki Nokki will work again.
1. Then put everything back again; “point C) till G)” in reverse.

When there is any question, please let me know.



